A logo with text and a symbol

Description automatically generated with medium confidence

SECTION 08 33 13.01 – COILING COUNTER SHUTTERS

GENERAL

ADMINISTRATIVE REQUIREMENTS

Pre-Installation Conference:

Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder] installer, and related trades.

Review: Project conditions, manufacturer requirements, delivery and storage, staging and sequencing, and protection of completed work.

SUBMITTALS

Action Submittals:

Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

Product Data: Manufacturer’s descriptive data and product attributes.

Samples: [Selection samples.] [Verification samples.]

Closeout Submittals:

Operation and Maintenance Data.

QUALITY ASSURANCE

Installer Qualifications: Minimum [2] [\_\_] years’ experience in work of this Section.

SYSTEM DESCRIPTION

Design Requirements: Positive and negative design wind loads in accordance with [ASCE 7.] [Building Code.] [\_\_\_\_.]

Operation: [Manual, push up.] [Reduced drive crank.]

WARRANTY

Manufacturer’s 2 year warranty against defects in materials and workmanship.

Manufacturer’s 40 year warranty for coating film integrity and 35 year warranty against chalking and fading of coating.

PRODUCTS

MANUFACTURERS

Contract Documents are based on Series 700 by ASTA America, [www.astaamerica.com](http://www.astaamerica.com/).

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

Galvanized Steel: ASTM A653/A653M, Structural Quality, G90 coating class.

\*\*\*\* OR \*\*\*\*

Aluminum:

Extrusions: ASTM B221.

Sheet: ASTM B209.

COMPONENTS

Curtain:

Material: 22 gage [galvanized steel.] [aluminum.]

Slat profile: Flat.

Slat size: 1-1/2 inch face width x ½ inch depth.

Endlocks: Ends of alternate slats fitted with endlocks.

Bottom bar: Extruded aluminum, single angle, with dual slide bolts and bottom astragal.

Locks: Keyed cylinder type; key locks [alike.] [differently.] [as directed by Owner.] Furnish [2] [\_\_] keys per lock.

Hood: [24 gage galvanized steel sheet] [0.0201 inch thick aluminum sheet], with closed ends.

Guides: Box shaped, extruded aluminum, two-piece configurations with soft brush guide runners, bell mouths, and head stop.

Barrel Assembly:

Barrel: Minimum 4-1/2 inch O.D. pipe; maximum 0.03 inch deflection per foot under full load.

Spring: Spring tension assembly supported within barrel by precision ball bearings.

Counterbalance: Curtain weight counterbalanced by oil-tempered, helically wound torsion springs, grease packed and mounted to steel torsion shaft.

Spring assembly life cycle: [20,000] [\_\_] cycles.

Head Plates: Steel plate.

FINISHES

Aluminum: [Clear anodized.] [Powder coated, [\_\_\_\_] color [to be selected from manufacturer’s full color range].

\*\*\*\* OR \*\*\*\*

Galvanized Steel: [Prime painted.] [Powder coated, [\_\_\_\_] color [to be selected from manufacturer’s full color range].

EXECUTION

INSTALLATION

Install in accordance with manufacturer’s instructions and approved Shop Drawings.

END OF SECTION